**NG SAMPLE APPENDIX 28/1: TRENCHLESS AND MINIMUM DIG TECHNIQUES**

*[Note to compiler: This should include:]*

**1** Identification of those drainage or service duct installations from Series 500 Appendix 5/1 and 5/2 that are to be constructed using trenchless or minimum dig techniques and schedule of permitted techniques; Product certificate requirements, for example, Irish Agrement Board certificate etc. *[2804.1]*;

**2** Information to be included in Contractor’s method statement including directions of bores or sequence of works, if to be specified *[2804.2]*;

**3**  Records of installation required (refer to Table NG 2804.1 plus any additional requirements) *[2804.5]*;

**4** Allowable ground movements if different from those specified in sub-Clause 2804.7 and the locations and periods when ground levels should be measured *[* *2807.7,2804.8]*;

**5**  Requirements for monitoring adjacent structures, pavements and services including conditions, line and level surveys and restrictions, if to be specified *[2804.9]*;

**6** Information on the presence and nature of known areas of contaminated ground including soil profile information *[2804.16]*;

**7** Requirements for existing manholes or chambers that are not to be reinstated *[2804.21]*;

**8** Permitted tolerances on alignment of pipeline if different from sub-Clauses 2805.10 and 2805.11 *[2805.10, 2805.11]*;

**9** The locations where existing drains, chambers or channels are to be connected to new drains, chambers or channels *[2805.19]*;

**10**  Details of reinstatement requirements for Minimum Dig Techniques, if to be specified *[2807.1]*;

**11** Details of sampling and testing required for cured in place lining technique *[2808.4]*;

**12** The content of the survey report, including number of copies and types should be specified *[2806.1, 2808.7 and 2808.9]*.