# NG Sample Appendices

NG Sample Appendix 23/1: Bridge Deck Expansin Joint Schedule

All bridge deck expansion joints shall satisfy the requirements of NRA Addendum to BD 33 'Expansion Joints for Use in Highway Bridge Decks'.

*[Notes to compiler: This schedule should list all bridge expansion joints in the Contract by type as described in Table 1 of BD 33/94 and give a cross-reference to the drawing number where the joint location is shown. The movement fringes of each joint should be given to enable the Contractor to propose an appropriate joint. Particular requirements for subsurface drainage, including the position and invert level of connections to surface water drains or soakaways should be given. Requirements for surface preparation and protection of metal components against corrosion should also be given].*

NG SAMPLE APPENDIX 23/2: SEALING OF GAPS SCHEDULE (OTHER THAN IN BRIDGE DECK EXPANSION JOINTS)

*[Note to compiler: This schedule should include all gap sealing such as joints between wing wall and abutment, etc. Typical aspects to be included are:]*

1. Joint types and references
2. Filler requirements
3. Sealant requirements
4. Water stop requirements
5. A cross-reference to the drawing number giving this or further information.